{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["产品目录"],"read":"whole","date_system":"1900"}

{"sheet":"产品目录","index":0,"n_rows":142,"n_cols":5,"rows_kept":142,"merged":[[0,0,0,4],[1,2,1,3],[2,0,15,0],[2,1,15,1],[2,2,2,3],[3,2,13,2],[3,4,13,4],[14,2,14,3],[16,0,20,0],[16,1,20,1],[16,2,18,2],[16,4,18,4],[19,2,20,2],[21,0,26,0],[21,1,26,1],[21,2,24,2],[25,2,26,2],[27,0,42,0],[27,1,42,1],[27,2,30,2],[27,4,30,4],[31,2,34,2],[31,4,35,4],[35,2,35,3],[36,2,36,3],[37,2,38,2],[39,2,42,2],[39,4,41,4],[43,0,47,0],[43,1,47,1],[43,2,45,2],[43,4,45,4],[46,2,46,3],[47,2,47,3],[48,0,65,0],[48,1,65,1],[48,2,65,2],[53,3,55,3],[53,4,55,4],[56,3,57,3],[56,4,57,4],[66,0,82,0],[66,1,82,1],[66,2,82,2],[66,4,80,4],[83,0,85,0],[83,1,85,1],[83,2,85,2],[86,0,92,0],[86,1,92,1],[86,2,92,2],[88,4,89,4],[93,0,97,0],[93,1,97,1],[93,2,97,2],[98,0,100,0],[98,1,100,1],[98,2,100,2],[101,0,114,0],[101,1,114,1],[101,2,114,2],[115,0,140,0],[115,1,140,1],[115,2,115,3],[116,2,133,2],[124,4,131,4],[134,2,134,3],[135,2,140,2],[141,2,141,3]]}
["附件1：\n            十三类消防产品自愿性认证产品目录"]
["序号","产品类别","产品名称",null,"认证依据标准"]
[1,"火灾报警产品","线型感温火灾探测器",null,"GB 16280"]
[null,null,"消防联动控制系统设备","消防联动控制器","GB 16806"]
[{"$nulls":3},"气体灭火控制器"]
[{"$nulls":3},"消防电气控制装置"]
[{"$nulls":3},"消防设备应急电源"]
[{"$nulls":3},"消防应急广播设备"]
[{"$nulls":3},"消防电话"]
[{"$nulls":3},"传输设备"]
[{"$nulls":3},"消防控制室图形显示装置"]
[{"$nulls":3},"消防电动装置"]
[{"$nulls":3},"消火栓按钮"]
[{"$nulls":3},"模块"]
[null,null,"防火卷帘控制器",null,"GA 386"]
[null,null,"城市消防远程监控产品","用户信息传输装置","GB 26875.1"]
[2,"消防通信产品","火警受理设备","火警受理信息设备","GB 16281"]
[{"$nulls":3},"火警调度机"]
[{"$nulls":3},"火警数字录音录时装置"]
[null,null,"消防车辆动态管理装置","消防车辆动态终端机","GA 545.1"]
[{"$nulls":3},"消防车辆动态管理中心收发装置","GA 545.2"]
[3,"火灾防护产品","防火涂料\n","饰面型防火涂料","GB 12441"]
[{"$nulls":3},"钢结构防火涂料","GB 14907"]
[{"$nulls":3},"电缆防火涂料","GB 28374"]
[{"$nulls":3},"混凝土结构防火涂料","GB 28375"]
[null,null,"防火封堵材料","防火封堵材料","GB 23864"]
[{"$nulls":3},"防火膨胀密封件","GB 16807"]
["    4 ","建筑耐火构件","防火窗","钢质隔热防火窗","GB 16809"]
[{"$nulls":3},"木质隔热防火窗"]
[{"$nulls":3},"钢木复合隔热防火窗"]
[{"$nulls":3},"其他材质隔热防火窗"]
[null,null,"防火门","钢质隔热防火门","GB 12955"]
[{"$nulls":3},"木质隔热防火门"]
[{"$nulls":3},"钢木质隔热防火门"]
[{"$nulls":3},"其他材质隔热防火门"]
[null,null,"防火锁"]
[null,null,"防火门闭门器",null,"GA 93"]
[null,null,"防火玻璃","隔热型防火玻璃","GB 15763.1"]
[{"$nulls":3},"防火玻璃非承重隔墙","GA 97"]
[null,null,"防火卷帘","钢质防火卷帘","GB 14102"]
[{"$nulls":3},"钢质防火、防烟卷帘"]
[{"$nulls":3},"特级防火卷帘"]
[{"$nulls":3},"防火卷帘用卷门机","GA 603"]
[5,"消防防烟排烟设备产品","防火排烟阀门","防火阀","GB 15930"]
[{"$nulls":3},"排烟防火阀"]
[{"$nulls":3},"排烟阀"]
[null,null,"消防排烟风机",null,"GA 211"]
[null,null,"挡烟垂壁",null,"GA 533"]
[6,"喷水灭火产品","喷水灭火产品","喷头（洒水喷头、水雾喷头、早期抑制快速响应（ESFR）喷头、扩大覆盖面积洒水喷头、水幕喷头、家用喷头）","GB 5135.1\nGB 5135.3\nGB 5135.9\nGB 5135.12\nGB 5135.13 \nGB 5135.15"]
[{"$nulls":3},"报警阀\n（湿式报警阀、干式报警阀、雨淋报警阀）","GB 5135.2\nGB 5135.4\nGB 5135.5"]
[{"$nulls":3},"水流指示器","GB 5135.7"]
[{"$nulls":3},"压力开关","GB 5135.10"]
[{"$nulls":3},"消防通用阀门","GB 5135.6"]
[{"$nulls":3},"感温元件（自动灭火系统用玻璃球）","GB 18428"]
[]
[]
[{"$nulls":3},"感温元件（消防用易熔合金元件）","GA 863"]
[]
[{"$nulls":3},"管道及连接件（沟槽式管接件）","GB 5135.11"]
[{"$nulls":3},"管道及连接件（消防洒水软管）","GB 5135.16"]
[{"$nulls":3},"减压阀","GB 5135.17"]
[{"$nulls":3},"加速器","GB 5135.8"]
[{"$nulls":3},"末端试水装置","GB 5135.21"]
[{"$nulls":3},"预作用装置","GB 5135.14"]
[{"$nulls":3},"自动跟踪定位射流灭火装置","GB 25204"]
[{"$nulls":3},"细水雾灭火装置","GA 1149"]
[7,"泡沫灭火设备产品\n","泡沫灭火设备产品\n","泡沫混合装置（压力式比例混合装置）","GB 20031 "]
[{"$nulls":3},"泡沫混合装置（平衡式比例混合装置）"]
[{"$nulls":3},"泡沫混合装置（管线式比例混合器、环泵式比例混合器）"]
[{"$nulls":3},"泡沫发生装置（低倍数空气泡沫产生器、高背压泡沫产生器、中倍数泡沫产生器）"]
[{"$nulls":3},"泡沫发生装置（泡沫钩管）"]
[{"$nulls":3},"泡沫发生装置（高倍数泡沫产生器）"]
[{"$nulls":3},"泡沫发生装置（泡沫喷头）"]
[{"$nulls":3},"泡沫泵"]
[{"$nulls":3},"专用阀门及附件（泡沫消火栓）"]
[{"$nulls":3},"专用阀门及附件（连接软管）"]
[{"$nulls":3},"泡沫喷射装置（泡沫炮）"]
[{"$nulls":3},"泡沫喷射装置（泡沫枪）"]
[{"$nulls":3},"泡沫消火栓箱"]
[{"$nulls":3},"轻便式泡沫灭火装置（半固定式（轻便式）泡沫灭火装置）"]
[{"$nulls":3},"闭式泡沫-水喷淋装置"]
[{"$nulls":3},"厨房设备灭火装置","GA 498 "]
[{"$nulls":3},"泡沫喷雾灭火装置","GA 834"]
[8,"干粉灭火设备产品\n","干粉灭火设备产品\n","干粉灭火设备","GB 16668 "]
[{"$nulls":3},"悬挂式干粉灭火装置","GA 602 "]
[{"$nulls":3},"柜式干粉灭火装置","GB 16668"]
[9,"气体灭火设备产品\n","气体灭火设备产品\n","高压二氧化碳灭火设备","GB 16669"]
[{"$nulls":3},"低压二氧化碳灭火设备","GB 19572"]
[{"$nulls":3},"卤代烷烃灭火设备","GB 25972"]
[{"$nulls":3},"惰性气体灭火设备"]
[{"$nulls":3},"悬挂式气体灭火装置","GA 13 "]
[{"$nulls":3},"柜式气体灭火装置","GB 16670"]
[{"$nulls":3},"油浸变压器排油注氮灭火装置","GA 835"]
[10,"灭火剂\n","灭火剂\n","泡沫灭火剂","GB 15308"]
[{"$nulls":3},"A类泡沫灭火剂","GB 27897"]
[{"$nulls":3},"水系灭火剂","GB 17835"]
[{"$nulls":3},"干粉灭火剂（BC干粉灭火剂、ABC干粉灭火剂、BC超细干粉灭火剂、ABC超细干粉灭火剂）","GB 4066                     GA 578"]
[{"$nulls":3},"气体灭火剂（二氧化碳灭火剂、七氟丙烷（HFC227ea）灭火剂、六氟丙烷（HFC236fa）灭火剂）","GB 4396\nGB 18614\nGB 25971"]
[11,"消防水带","消防水带\n","有衬里消防水带\n(塑料衬里消防水带除外)","GB 6246"]
[{"$nulls":3},"消防软管卷盘","GB 15090"]
[{"$nulls":3},"消防吸水胶管","GB 6969"]
[12,"消防给水设备产品","消防给水设备产品","车用消防泵（车用消防泵）","GB 6245"]
[{"$nulls":3},"车用消防泵（消防球阀）","GA 79"]
[{"$nulls":3},"消防泵组","GB 6245"]
[{"$nulls":3},"室外消火栓（室外消火栓）","GB 4452"]
[{"$nulls":3},"室外消火栓（消防水鹤）","GA 821"]
[{"$nulls":3},"室内消火栓","GB 3445"]
[{"$nulls":3},"消防水泵接合器","GB 3446"]
[{"$nulls":3},"消防枪炮（消防水枪）","GB 8181"]
[{"$nulls":3},"消防枪炮（泡沫枪）","GB 25202"]
[{"$nulls":3},"消防枪炮（干粉枪）","GB 25200"]
[{"$nulls":3},"消防枪炮（脉冲气压喷雾水枪）","GA 534"]
[{"$nulls":3},"消防枪炮（消防炮）","GB 19156\nGB 19157\n"]
[{"$nulls":3},"分水器和集水器","GA 868"]
[{"$nulls":3},"消防接口","GB 12514.1\nGB 12514.2\nGB 12514.3\nGB 12514.4"]
[13,"消防装备产品","正压式消防空气呼吸器",null,"GA 124"]
[null,null,"消防员个人防护装备\n","消防头盔","GA 44"]
[{"$nulls":3},"消防员灭火防护头套","GA 869"]
[{"$nulls":3},"消防员灭火防护服","GA 10"]
[{"$nulls":3},"消防员隔热防护服","GA 634"]
[{"$nulls":3},"消防员化学防护服装","GA 770"]
[{"$nulls":3},"消防手套","GA 7"]
[{"$nulls":3},"消防员灭火防护靴","GA 6"]
[{"$nulls":3},"消防腰斧","GA 630"]
[{"$nulls":3},"安全绳","GA 494"]
[{"$nulls":3},"安全带"]
[{"$nulls":3},"安全钩"]
[{"$nulls":3},"上升器"]
[{"$nulls":3},"抓绳器"]
[{"$nulls":3},"便携式固定装置"]
[{"$nulls":3},"下降器"]
[{"$nulls":3},"滑轮装置"]
[{"$nulls":3},"消防员呼救器","GB 27900"]
[{"$nulls":3},"正压式消防氧气呼吸器","GA 632"]
[null,null,"消防摩托车",null,"GA 768"]
[null,null,"抢险救援产品\n","消防斧","GA 138"]
[{"$nulls":3},"消防救生气垫","GA 631"]
[{"$nulls":3},"消防梯","GA 137"]
[{"$nulls":3},"消防移动式照明装置","GB 26755"]
[{"$nulls":3},"消防救生照明线","GB 26783"]
[{"$nulls":3},"移动式消防排烟机","GB 27901"]
[14,"消防车","消防车",null,"GB7956.1\nGB7956.2\nGB7956.3\nGB7956.6\nGB7956.12\nGB7956.14\nGA 39"]